

                     Read1st for Marvell Flash Image Package
                     --------------------------------------
                **** ONLY FOR 277x/278x/28xx Series Adapters ****



 1. Contents Of Flash Package
--------------------------------

The files contained in this Flash image package are zipped into a file that 
 will expand to provide the following versions for the 28xx Series Adapters.

*  Flash Image Version 10.10.08 to support A1 only

   MH101008.BIN contains for common:
   ---------------------------------
     Bootcode EFI	7.41 (signed)
     PEP SoftROM	3.00.13
     PEP Brd Cfg 4P	03.00.00
     PEP Brd Cfg 2P	03.01.00
     PEP Brd Cfg 1P	03.02.00
     FC Brd Cfg	4P	03.00.03
     FC Brd Cfg	2P	03.00.02
     FC Brd Cfg	1P	03.00.02
   
     FC Firmware	9.15.17
     PEP Firmware	3.01.39
     PCIe Serdes	03.00.07
     MPI FW 		3.04.04

     Preload FWA 4P	03.03.09
     Preload FWA 2P	04.01.16
     Preload FWA 1P	04.05.07
	 
	 PLDM MCTP  	1.00.00
	 PLDM MCTP  	1.01.00
     
     
*  Eflash tool v1.29

2. Flash Image Update Methods
--------------------------------

Install the latest driver and QConvergeConsole CLI.  Use Flash Update Option from CLI to update the MBI (*.bin) file from the Multiboot Image package. 

  * Refer to QConvergeConsole , Adapter user guides for more details.

