

                     Read1st for Marvell Flash Image Package
                     --------------------------------------
                   **** ONLY FOR 268x/269x/27xx Series Adapters ****



 1. Contents Of Flash Package
--------------------------------

The files contained in this Flash image package are zipped into a file that 
 will expand to provide the following versions for the 268x/269x/276x Series Adapters.

*  Flash Image Version 10.04.07

   BK100407.BIN contains:
   ----------------------
     Bootcode FC
       FC BIOS       v3.68
       FC FCode      v4.11  (Initiator)
       FC FCode      v4.10  (Target)
       FC EFI        v7.32   (re-signed)
       MPI	         v3.03.09
     FC Firmware     v9.15.01
     PEP Firmware(Quad-port)        v1.1.44
     PEP Firmware(Single/Dual port) v2.1.30
     PEP SoftROM(Quad port)         v1.0.16
     PEP SoftROM(Single/Dual port)  v2.0.11
	 PLDM MCTP SPEC v1.01.00
	 PLDM MCTP SPEC v1.00.00
     
     EFlash tool  v1.26


     
2. Flash Image Update Methods
--------------------------------

Install the latest driver and QConvergeConsole CLI.  Use Flash Update Option from CLI to update the MBI (*.bin) file from the Multiboot Image package. 

  * Refer to QConvergeConsole , Adapter user guides for more details.

